GD03 Logger v1.0

Requirements:
- Microsoft Excel installed
- Windows 10/11

Usage:
1. Verify that gas flow is being detect
2. Connect the GD03 Gas Flow Meter to the included 9V power supply and the USB cable to the PC.
3. Launch GD03_Logger.exe.
4. Click "Port Finder".
5. Click "Start".

The software creates a live Excel logger with real-time chart.