GD03 Logger v2 from 17.06.2026

Requirements:
- Microsoft Excel installed
- Windows 10 or 11

Usage:
1. Verify that gas flow is being detected.
2. Connect the GD03 Gas Flow Meter to the included 9V power supply and connect the USB cable to the PC.
3. Launch GD03_Logger.exe.
4. Click "Port Finder".
5. Click "Start".

The software provides live Excel logging with a real-time chart and automatically archives raw data in CSV format.
